**Release Notes**

|  |  |  |
| --- | --- | --- |
| **Version** | **Comment** | **Supported SVC** |
| **1.1.1 Compatibility**:  ROBOGUIDE v9.40 P/60  Tablet TP V1.30 | New command “Set Workspace”  Option: R648 User Socket MSG mandatory Option: R640 MROT optional (when joint move used to reach grasp position) | TCP/IP Protocol version 4 |
| **1.1.0**  **Compatibility**:  ROBOGUIDE v9.40 P/60  Tablet TP V1.30 | SVC protocol version 4 supported  Support for industrial robots on R30iB controller  Option: R648 User Socket MSG mandatory Option: R640 MROT optional (when joint move used to reach grasp position) | TCP/IP Protocol version 4 |
| **1.0.0**  **Compatibility**:  ROBOGUIDE v9.40 P/53  Tablet TP V1.30 | Initial release Option: R648 User Socket MSG mandatory Option: R640 MROT optional (when joint move used to reach grasp position) | TCP/IP Protocol version 3 |